F-LE-85 Rev July 9, 2025

**High-Performance Alloys Product Statement**

Products Include: High Performance Alloys: 35N LT®™, MP35N®, FWM®™ 1058, FWM®™ 1537, Alloy 31, Alloy 41, Alloy 600, Alloy 625, Alloy 718, Alloy 901, Alloy 902, Hastelloy® Alloy B, Hastelloy®/Alloy-X, INCONEL® Alloy 601, Haynes® 188, Haynes® 230™®, Haynes® Alloy C-263, Alloy X-750, Alloy C-276, Alloy C-22, NI 200, Nimonic® 90, ULTIMET®, CBX Cupron® Gr 1, CBX Cupron® Gr 2, Tophet® A, and HyMu 80.

**This statement excludes research and development and prototype projects and material.**

Fort Wayne Metals Research Products, LLC (FWM) product, when shipped, meets or exceeds the following statements:

**EU RoHS, RoHS 2, RoHS 3 Compliance (EU Directive 2015/863):**

The products listed above do not contain intentionally added Substances above the RoHS, RoHS 2, RoHS 3 stated concentration limits.

**EU REACH Compliance (Regulation EC/1907/2006):**

The products listed above do not contain intentionally added REACH Substances of Very High Concern (SVHC) as listed in the June 25, 2025 (250SVHC) list, in concentrations above 0.1% weight by weight.

REACH Annex XIV: The products listed above do not contain substances listed on the REACH Authorization List.

REACH Restriction List (Annex XVII): The above listed products contain Nickel.

|  |  |  |
| --- | --- | --- |
| Nickel Content: |  |  |
| Alloy 41: 46% w/w | Alloy 600/ Inconell 600: 72.0% min w/w | Alloy 625: 58% w/w |
| C276 Alloy: Balance | Alloy X, Hastelloy X: Balance | Alloy X750: 70.0 % max w/w |
| Evanohm R / Alloy 800: 71% w/w | Nickel 200: 99% min w/w | Nickel 270: 99.9% max w/w |
| Nikrothal® 60: 57 – 60% w/w | Nimonic 90: 51% w/w | SX500: 46 – 75% w/w |
| Tophet® Alloy 30: 70% w/w | Tophet® Alloy A: 77 – 79% w/w | Tophet Alloy C: 79% w/w |
| Waspaloy: 51% w/w | HyMu 80: 50 – 100% w/w | CBX Cupron: 44% w/w |
| ULTIMET®: 9% w/w | 35N LT: 33 – 37 % w/w | MP35N: 33 – 37% w/w |
| FWM1058: 15 – 16% w/w | FWM1537: 1% max w/w |  |

**Latex:**

FWM does not use or intentionally add natural rubber latex for the production of the above products.

**Bisphenol A (BPA):**

FWM does not use or intentionally add BPA for the production of the above products.

**Phthalates:**

FWM does not use or intentionally add phthalates for the production of the above products.

**Nanomaterial:**

FWM does not use or intentionally add nanomaterials as defined in Regulation (EU) 2017/745 for the production of the above products.

**EU MDR CMR & Endocrine Disrupting Substances:**

The products listed above do not contain endocrine disrupting substances or carcinogens, mutagens, or reproductive (CMR) toxins category 1A or 1B as listed in Annex VI to CLP ATP22 (Regulation (EU) 2024/2564 & 2022/692) in concentrations above 0.1% weight by weight (w/w), except for Cobalt.

|  |  |  |
| --- | --- | --- |
| Cobalt Content: |  |  |
| 35N LT™: 29-39% max w/w | Alloy 600: 0-1% max w/w | Haynes® C-263: 0-20% max w/w |
| MP 35N®: 30-39% max w/w | Alloy 625 0-1% max w/w | Alloy X750: 0-1% max w/w |
| FWM® 1058: 36.5-45% max w/w | Alloy X/Hastelloy®: 0.5-2.5% max w/w | Alloy C276: 0-2.5% max w/w |
| FWM®™1537: 58.8-69% max w/w | Haynes® 188: 0-39% max w/w | Nimonic® 90: 15-21% max w/w |
| Alloy 41: 10-12% max w/w | Haynes® 230™®: 0-5% max w/w | CBX Cupron® 0.1-1% max w/w |

**Polyvinyl Chloride (PVC):**

FWM does not use or intentionally add polyvinyl chloride (PVC) for the production of the above products.

**EU Biocidal Products Regulation:**

FWM does not use or intentionally add biocidal products identified in Regulation (EU) 528/2012 for the production of the above products.

**Antimicrobial Agents:**

While we have “cleaning processes”, they are not intended to be a final clean to any standard but rather an in-process step to remove excess processing agents. The biocompatibility of our products is not certified from our facility and must be evaluated through clinical studies conducted by the final device manufacturer.

**Human Derived Material:**

FWM does not use or intentionally add Human Derived Material as defined in EU Directive 2004/23/EC for the production of the above products.

**EU Persistent Organic Pollutants (POPs):**

FWM does not use or intentionally add persistent organic pollutants (POPs) as defined in Regulation (EU) 2019/1021 and Regulation (EU) 2022/2400 for the production of the above products.

The information in this statement is based on information provided by our suppliers and from random sample testing by outside accredited laboratories.

Fort Wayne Metals Research Products, LLC

Product Regulatory Team